# Scripting

parameter values can be changed automatically with the scripting window. It is started with the button from the parameter editor.

The script is written into a textfile, which is generated by an arbitrary editor. The textfile must be in csv-format with the following layout:

The script contains 5 columns, which are separated by a semicolon.

1. Time in seconds

2. value of the parameter without unit.

3. device name. It must be either Short Name (Parameter 0005) or the address for example "UDP: 10.49.1.42:2904".

4. parameter id

5. sub id

An example looks as following:

5;0;CAN-IO;3104;0

10;1;CAN-IO;3104;0

In this example the parameter 3104 is set to 0 after 5 seconds past pressing the start button. 5 seconds later (10 seconds after start) the parameter is set to 1.

If the button loop is pressed, the script restarts after the last line.