# Cross-Communication (134)

The cross-communication of the inverter has reported an error.

The cause of the error can be detailed by the Sub-ID:

### 0 - Timeout

No message of the communication partner has arrived within set time.

### 1 - Wrong Data received

An invalid data packet has been received.

### 3 - Other Device not in Run State

The communication partner has left the running state. The error can only occur if previously were both devices in running state.

### 4 - Timeout for Run State

The communication partner has not switched in running state within a set time during power on.

## Fehleraktion

Ein Not-Aus wird durchgeführt.

## Troubleshooting

The error can be acknowledged by an Error-Reset.