# Calibration

In this section the voltage and current measurements of the converter is calibrated.

Please choose first which sensors you wish to calibrate. Also tell if sufficiently accurate voltage or current values are available via Modbus.

If these values are not available via Modbus, you need to determine these values through own measurements. You will be asked during the procedure to perform these measurements and enter these values.

The drive is feed with current and could make small movements.

You can interrupt the calibration at any time and start over again.