# Parameterinterface (118)

The parameter interface for the communication between device and PC is disturbed.

The cause of the error can be detailed by the Sub-ID:

### 0 - Cannot Init Parainterface: Bind failed

The initialization of the parameter interface via Ethernet failed.

### 1 - Cannot Init Parainterface: Listen failed

The initialization of the parameter interface via Ethernet failed.

### 2 - Burst-Frame too big

To many bytes are transferred on the Ethernet interface.

### 3 - Send-Buffer Full

The transmit buffer has overflowed.

### 4 - Cannot establish connection: Out of memory

The main memory is no longer sufficient to handle an incoming connection request.

### 5 - Parameterset Change not allowed while running

The change of parameter sets is not allowed while inverter is running.

## Fehleraktion

Durch diesen Fehler wird keine Aktion ausgeführt.

## Troubleshooting

The error can be acknowledged by a restart of the device.