# Temperature (108)

A temperature has exceeded the set limit.

The cause of the error can be detailed by the Sub-ID:

### 0 - Controlprint over temperature

The temperature of the control board is above the limit in parameter 1120.

### 1 - Modstack over temperature

The temperature of the modstack is above the limit in parameter 1130.

### 2 - Phase U over temperature

The temperature of the motor in phase U is above the limit in parameter 1280. The motor temperature is transmitted via modbus by plc.

### 3 - Phase V over temperature

The temperature of the motor in phase V is above the limit in parameter 1280. The motor temperature is transmitted via modbus by plc.

### 4 - Phase W over temperature

The temperature of the motor in phase W is above the limit in parameter 1280. The motor temperature is transmitted via modbus by plc.

## Fehleraktion

Ein Not-Aus wird durchgeführt.

## Troubleshooting

The error can be acknowledged by an Error-Reset.