# Graph

parameter values can be recorded and shown on the time scale with the graph vbalue. this is only useful for slow changing values like tmeperatures, because of the low update cycle of appr. 2 Hz.

The values can be added with the context menu of the parameter.

# Menü

### File

The graph can be exported as comma separated values into a csv-file.

### Signals left / right

All signals can be displayed either on the left or on the right side of the window. Both axis have a different scaling and are independent from each other. The scaling is set automatically dependant of the minimum and maximum value.

### Time

The x-axis is autoscaled, too. The whole measurement cycle is displayed. Its range can be selected with the selector field to reduce the scaling ox the time axis.

### Sample Time

The sample time can be reduced with this selection field. normally the highest possible sampling time is selected.