# TFTP (132)

The access from PC to the memory card is disturbed.

The cause of the error can be detailed by the Sub-ID:

### 0 - Cannot create TFTP Socket

When initializing the Ethernet-socket for TFTP connection can not be created. Check Ethernet-connection.

### 1 - Cannot bind TFTP Port

When initializing the Ethernet-port for TFTP connection can not be reserved. Check Ethernet-connection.

### 2 - Error while processing TFTP Request

The PC has send an error message while connecting. Check Ethernet-connection.

### 3 - Cannot Close actual File

The transmitted file can not be closed.

### 4 - Error while reading file

There was an error while reading the file to be send. The error occurs only in combination with SD-card error. In this error the exact cause of the error of the card driver will be reported.

### 5 - Cannot Seek in actual File

There was an error while reading the file to be send. The error occurs only in combination with SD-card error. In this error the exact cause of the error of the card driver will be reported.

## Fehleraktion

Durch diesen Fehler wird keine Aktion ausgeführt.

## Troubleshooting

The error can be acknowledged by an Error-Reset.