# Supply (103)

One of the power supplies has left the allowable range.

The cause of the error can be detailed by the Sub-ID:

### 0 - 3,3 V over Voltage

The 3,3 V voltage is greater than 3,465 V.

### 1 - 3,3 V under Voltage

The 3,3 V voltage is lower than 3,135 V.

### 2 - 5 V over Voltage

The 5 V voltage is greater than 6,0 V.

### 3 - 5 V under Voltage

The 5 V voltage is lower than 4,5 V.

### 4 - 15 V over Voltage

The 15 V voltage is greater than 16,5 V.

### 5 - 15 V under Voltage

The 15 V voltage is lower than 12,75 V.

### 6 - 24 V over Voltage

The 24 V voltage is greater than 27,6 V.

### 7 - 24 V under Voltage

The 24 V voltage is lower than 21,6 V.

## Fehleraktion

Der Umrichter wird abgeschaltet.

## Troubleshooting

There are different error causes:

- Voltage fluctuations in the supply voltage

- EMC irradiation in the supply voltage or the voltage measurement

- Damage of the power supply

- Damage of the DC-DC converter

The error can be eliminated by rebooting. If the error occurs again the unit and/ or the power supply should be replaced.