# Watchdog (115)

The device has a watchdog timer, which must be reset by the software periodically.

If not, e.c. because of a software error, an interrupt is executed and at repeated triggering of the watchdog a reset is initiated.

The cause of the error can be detailed by the Sub-ID:

### 0 - Watchdog IRQ

The watchdog has triggered the first time. As a result the device is switched off.

### 1 - Reset by Watchdog

The watchdog has triggered a reset. The device has restarted.

## Fehleraktion

Ein Not-Aus wird durchgeführt.

## Troubleshooting

The error can be acknowledged by a restart of the device.

The error indicates a problem in the firmware of the converter.

Please contact the development department.