# Snapshot (129)

An error has occurred while creating a snapshot file.

The cause of the error can be detailed by the Sub-ID:

### 0 - Cannot Create Snapshot-File

The snapshot file can not be generated. The error occurs only in combination with SD-card error. In this error the exact cause of the error of the card driver will be reported.

### 1 - Cannot Write to Snapshot-File

The snapshot file can not be written. The error occurs only in combination with SD-card error. In this error the exact cause of the error of the card driver will be reported.

### 2 - Cannot Close Snapshot-File

The snapshot file can not be closed. The error occurs only in combination with SD-card error. In this error the exact cause of the error of the card driver will be reported.

### 3 - Cannot Open Snapshot-Dir

The snapshot file can not be opened. The error occurs only in combination with SD-card error. In this error the exact cause of the error of the card driver will be reported.

Normally during start the micro controller the SD card is read and checked whether the necessary directories exist. If not these can be created. The error should be corrected automatically after a reboot.

## Fehleraktion

Durch diesen Fehler wird keine Aktion ausgeführt.

## Troubleshooting

The error can be acknowledged by an Error-Reset.